
|  |  |  |  |
| --- | --- | --- | --- |
| **Sediment** | **Flow time (s)** | **Water recovered (mL)** | **Permeability (mL/s)** |
| Sand | 54.8 s | 19 mL | 0.347 mL/s |
| Gravel | 5.4 s | 44 mL | 8.148 mL/s |
| Gravel & Sand | 88.7 s | 30 mL | 0.338 mL/s |

**pH: 7**



**Soil Make-Up:** 83% sand, 13% silt, 4% clay